USB 1.1 Human interface device (HID)

The USB commands are variable length data packets that are sent with the least significant byte first.

DVI:

912\*1140 pixel \* 24-Bit bitmap \* 120 Hz

=1,039,680 \* 3 Byte \* 120 = 374,284,800 Byte / sec = 374mb/s